About “Quick reference manual for the installation of Vigor2000 isdnRouter”
This “Quick reference manual for the installation of Vigor2000 isdnRouter” is designed to assist users in using the DrayTek Vigor2000 isdnRouter. Information in this document has been carefully checked for accuracy; however, no guarantee is given as to the correctness of the contents. The information contained in this document is subject to change without notice. Should you have further inquiries, please feel free to contact support@draytek.com.tw . For latest product info and latest features, please visit www.draytek.com.tw. 

Revision
Ver. 1.0, September 1999

Copyright
This publication contains information that is protected by copyright. No part of it may be reproduced, transmitted, transcribed, stored in a retrieval system, or translated into any language without written permission from the copyright holders.

Copyright © 1999
DrayTek Corporation. All rights reserved.

Trademarks
Microsoft is registered trademark of Microsoft Corp. Windows, Windows 95, Windows 98, Windows NT and Windows2000 are trademarks of Microsoft Corp. Other trademarks and registered trademarks of products referred to in this manual are the properties of their respective holders.

How To Become A Registered Owner
Web registration is preferred. Please visit the following WEB site: http://www.draytek.com.tw/registration.htm
Alternatively, you can fill in the registration card and mail it to the address found on the reverse side of the card. Registered owners will receive future product and update information.

Safety Instructions
�o	You shall get the installation guide as you use the ISDN router.  Please read the installation guide thoroughly before you set up the router.
�o	The ISDN router can be used only with a BRI (basic rate interface) ISDN line.
�o	The ISDN router is a complicated electronic unit that may be repaired only be authorized and qualified personnel.  Please do not try to open or repair the ISDN router yourself.
�o	Please do not place the ISDN router in a damp and humid place such as a bathroom.
�o	The ISDN TA shall be used in a sheltered and non-slip place within a temperature range of +5 to +40 Celsius degree.
�o	Please keep the wrap bag of ISDN router and the clip binding the cable out of reach of children.  Because small children and babies will be in danger of choking if they put small objects in their mouth.
�o	Please do not expose the ISDN router to direct sunlight or other heat sources.  The housing and electronic components may be damaged by direct sunlight or heat sources.
�o	Once you would like to get rid of the ISDN router, please follow the local regulations on conservation of the environment.  

Warranty
We warrant to the original end user (purchaser) that this Vigor2000 isdnRouter is free from any defects in workmanship or materials for a period of up to two (2) years from the date of purchase from the dealer. Please keep your purchase receipt in a safe place because it serves as proof of date of purchase.
During the warranty period, and upon proof of purchase, should the Vigor2000 isdnRouter have indications of failure due to faulty workmanship and/or materials, we will, at its discretion, repair or replace the defective products or components without charge for either parts or labor, and to whatever extent it shall deem necessary to restore the Vigor2000 isdnRouter or components to proper operating condition. Any replacement will consist of a new or re-manufactured functionally equivalent product of equal value, and will be solely at the discretion of us. This warranty shall not apply if the Vigor2000 isdnRouter is modified, misused, tampered with, damaged by an act of God, or subjected to abnormal working conditions.
The warranty does not cover the bundled or licensed software of other vendors.  The defects which do not significantly affect the value of the usability of the Vigor2000 isdnRouter will not be covered by the warranty.
Further, we reserve the right to revise the manual and online documentation and to make changes from time to time in the contents hereof without obligation to notify any person of such revision or changes.

Y2K compliance
We confirm that Vigor2000 isdnRouter recognize the year 2000 as a leap year and accept February 29, 2000 as a valid date. The mathematical and logical functionality, and preciseness of DrayTek's isdnVigor2000 will not be affected as a result of turn of the century.

The Declarations of CE Marking
The Vigor2000 isdnRouter has been approved for connection to the Public Switched Telecommunication Network using interfaces compatible with ITU-TSS recommendation I.430 (Basic Rate ISDN user access). The Vigor2000 isdnRouter complies with the following directives:

1. The Council Directive 89/336/EEC of 3 May 1992 on the approximation of the laws of the Member States relating to Electro Magnetic Compatibility. (EMC Directive)

2. The Council Directive 92/31/EEC of 28 April 1992 amending directive on the approximation of the laws of the Member States relating to Electro Magnetic Compatibility.

3. Council Directive 91/263/EEC of 29 April 1991 on the approximation of the laws of the Member States concerning telecommunication terminal equipment. (The Telecom Terminal Equipment Directive)

4. 93/68/EEC of 22 July 1993 amending the Directives 89/336/EEC, 91/263/EEC, and 92/31/EEC. (Marking Directive)

5. Council Directive 73/23/EEC and 93/68/EEC of 26 December 1996 on the harmonization of the laws of the Member States relating to electrical equipment designed for use within certain voltage limits. 

What does Vigor2000 isdnRouter offer?
��	Convenient Internet Access for home users and the staff of a small office:
It offers an IP router with web-user-interface configuration, 6-port 10BaseT Ethernet hub, one uplink port (expandable for business growth), and one ISDN connection to one entire home network or small office for Internet via one single ISDN BRI line. 

��	Virtual TA for communications applications:
Because the Vigor2000 isdnRouter also functions as a CAPI server for your network, the fax and file transfer provided by communications applications can be deployed at every computer through ISDN network without the physical presence of an ISDN terminal adapter in the PC.

��	Reliable Remote Access for telecommuting
The members of a home or the staff of a small office can dial back from outside to the home-LAN or office-LAN to access information in a database on the LAN. 

��	Simultaneous access to Internet for multiple users
The less Internet cost, the better joy for many users of LAN to surf Internet through a single access account subscribed from your local Internet Service Provider (ISP). 

��	Built-in Ethernet Hub and Uplink for connecting to multiport hub
Accommodate flexibility for growing business or adding new home members to use ISDN Internet.

Contents
1.	Introduction
Unpacking Your Vigor2000 isdnRouter
The LED indicator&back panel

2.	Chart of cable connection of Vigor2000 isdnRouter

3.	Software Installation Guide for Vigor2000 isdnRouter

1. Introduction
The Vigor2000 isdnRouter provides multiple users with the efficient and reliable access over a single ISDN line to the Internet and corporate LAN for using E-mail, sharing documents, Web surfing, and file transfer.  Moreover, the provision of a built-in six-port 10BaseT Ethernet hub and one uplink port  may give cost-effective workgroup connectivity over Ethernet.

In addition to improving the productivity of employee, flexible telecommuting access, the affordable management cost, Vigor2000 isdnRouter accommodates room for business growth from 6-7 computers to more.  The smart solutions of DrayTek Vigor2000 isdnRouter brings SOHO into “easy to setup and use”,” instant Internet and Intranet connectivity”,” high interoperability and good security for network management”.

Chart of Applications:

Unpacking Your Vigor2000 isdnRouter:

Your Vigor2000 isdnRouter should come with the equipment listed below. If any item is missing or damaged, please contact your dealer or DrayTek Customer Service Department immediately.

��	One (1) Quick reference manual for the installation of Vigor2000 isdnRouter
��	One (1) warranty/registration card
��	One (1) RJ-45 ISDN telephone cable (black color)
��	One (1) AC/AC power adapter (black color)
��	One (1) Console cable (gray color)
��	One (1) 10BaseT Lan cable (blue color) for connection to computer or to hub
��	One RJ45 to RS232 (9 pin converter) for console cable 
Dimensions (cm) of the ISDN router: (L) 21.8 X(W) 15.8 X (H) 3.6
Weight:  399 grams
Maximum Power: 10W
Power Adapter: AC adapter, Class2 transformer, input is230VAC 50Hz, output is 15VDC 600mA

Chart of power adapter, cables, and rear panel of the ISDN router:

The Operating System Compatibility:
Windows 95/98/NT/2000
Mac OS
Linux or other UNIX clone

The LED Indicators & Back Panel

Portion	LED	Function	Corresponding rear-panel Port	Color	
System	ACT	Blinks when the power is supplied to the router and router software is running.	PWR(power) port and router software	Green	
ISDN	LINK	On when the ISDN network is set up 	ISDN port	Green	
ISDN	B1
	On when there is successful remote ISP connection and when the B1 channel delivers a packet	ISDN port	Green	
ISDN	B2	On when there is successful remote ISP connection and when the B2 channel delivers a packet	ISDN port	Green	
Ethernet Lan	COL	Blinks when there is collision of packets within the Ethernet	P1to P6 and Uplink port	Yellow	
Ethernet Lan	Pn
N=1 to 6	1.On when the computer is connected and there is no packet.
2. Blinks when the packet is receiving/sending through hub or connected computer	Pn port
N=1 to 6	Green	
Ethernet Lan	Uplink	lights when the router is connected to one hub	Uplink port	Green	

Requirements for using Internet via ISDN
�o	Please firstly get the Basic Rate Interface (BRI) ISDN from local Telcos.
�o	You shall subscribe the Internet account from Internet Service Provider (ISP). 

How you connecting the cable of Vigor2000 isdnRouter with computers, hub, ISDN NT1

Step 1.:  Connect the attached power adapter cord (black color) to the power socket on the router rear panel.
Step 2:  Connect the attached console cable (gray color) to the console port on the router rear panel for setting up the ISDN router.
Step 3:  Connect the ISDN RJ45 cable (black color) to the ISDN port on the router rear panel and connect the other end of the cable to an ISDN NT1 wall jack.
Step 4:  If you would like to connect the ISDN router to the network of computers, you may use the attached 10BaseT Lan cable (blue color) to connect the router and computer or an individual hub.

Note: Once you need more 10BaseT Lan cable for computers or hub, please purchase it locally in accordance with your need.																

Following chart is the Uplink port and six-port 10BaseT Ethernet hub are full loaded: