How to establish Web / FTP Servers via V2600?

Step 1 : Enable Router to Accept Accessing From Internet

Check Allow management from the Internet.

System Management >> Management Setup

Step 2 : Make the router always on line ( for PPPoE/PPPoA mode users)

Setting Idle Timeout as -1 or just check on "Always On" , it will force router to

connect to internet when the line is drop.

Quick Setup >> Internet Access Setup >> PPPoE/PPPoA

Step 3 : Get dynamic DNS service ( for PPPoE/PPPoA mode users)

The router supports the following DDNS servers. You can register an account and

hostnames from the servers. For example, you can register one from

http://www.dyndns.org.

Advanced Setup >> Dynamic DNS Setup >> Dynamic DNS Account Setup

After getting an account and a hostname, please input the texts and do not forget to

enable it.

Advanced Setup >> Dynamic DNS Setup >> Dynamic DNS Account Setup

You need also check Enable Dynamic DNS Setup

Advanced Setup >> Dynamic DNS Setup

For this example, you can ping the domain name to make sure it works.

You also need to check if the IP of your domain name is same as router's IP address.

System Management >> Online Status

Step 4 : Installing Web/FTP server

There are many free Web servers and FTP servers. For example, AN HTTPD is a

simple free Web server for Win95/98/NT/2000. And Apache Web Server is a quite

famous free Web server for unix system. TYPSoft FTP Server is a free FTP server for

Win95/98/NT/2000. You can find them in internet. Get the servers and install them in

the indicated PC.

Step 5 : Redirect accessing port from router to the indicated PC

Following is the well known ports list. It is a quite important information to do port

redirection.

Advanced Setup >> NAT Setup >> View Well-Known Ports List

It is better to use fixed IP for indicated PC. The default gateway is 192.168.1.1 and the

dynamic IP assigned is from 192.168.1.10. So you can choose the IP between

192.168.1.2 and 192.168.1.9 as the fixed IP address of the indicated PC.

Basic Setup >> Ethernet TCP/IP and DHCP Setup

According the ports list, you can redirect the service port to the indicated PC's port.

Advanced Setup >> NAT Setup >> Configure Port Redirection Table

Now you can provide your Web/FTP server in internet for others. The illustration is as

below.