Main | Quick Start Wizard | Documents | Tools | Tips | Utilities
I do not know what VPI/VCI, Encapsulation Type, protocol is. How can I configure V2600? For ADSL service, it needs to set VPI, VCI, Encapsulation mode, Protocol ( PPP service or MPoA service)..... Most of the time, your ISP can provide these message for you. Then, you can directly use these message for setting ATM/DSL on V2600 . However, some ISP will not give the said information to you. Consequently, V2600 provides "Auto detect ATM/DSL settings" function for you to auto-configure ATM/DSL setting. When you enter the auto-configure procedure, the screen will ask you to select your country. V2600 has made different country's databases to speed up the procedure. If your country is not in the list, you still can use this function but it may take much longer time to finish auto-configure procedure. If this function can not detect your settings,please contact your ISP to ask them to offer you these messages (e.g. VPI/VCI value).
Copyright (c) 2003, DrayTek Corp. All Rights Reserved.