Main | Quick Start Wizard | Documents | Tools | Tips | Utilities
How can I configure my V2600 in the bridge mode when user use PPPoE? 1.Please first set as the following photo: 2.Enable PPPoE pass-through. You have to enable "For Wired LAN" item,if you allow Wired LAN users to use this function. You have to enable "For Wireless LAN" item,if you allow Wireless LAN users to use this function. 3.And then pc behind router could dial up via dial-up software. If you want to put a router behind V2600,you could use PPPoE to dial out. Note: PPPoE pass-through function has been disabled for security issue.
Copyright (c) 2003, DrayTek Corp. All Rights Reserved.