/============================================================
//	Program: CMS
//	Version: 3.2.0
//	Date:  10/03/2008
//============================================================
[New functions]
1.  Support DVR user management.
2.  Support recording videos into multiple HDDs and circular recording.
3.  Config dialog will be closed automatically if it is idled for more than 5 minutes.
4.  Get client device network status and show message (3~5min).
5.  Added Site Tree expand and collapse function.
6.  Added Auto Reconnect function.
7.  Add AXIS and VIVOTEK DOME CONTROL.
8.  Each user has its own layout setting file.
9.  Enable CMS to show images of cameras even if they are covert at DVR site. 
10. List DVR System Log.
11. Detect the network state.
12. Search UPNP devices.
13. Support CH Products joystick control.
14. Brand-new interface.
15. Support new NH Series API function.
16. Support new NH Series Stream Server.
17. Support DG8X MJPEG video.

[Change]
1.  Improved CMS Player PB & PPS.
2.  If the time interval of a DRV file is less than three seconds, CMS player will not be able to successfully convert this file.
3.  Auto Schedule Record or Site Record after Auto Reconnect.
4.  Changed functions regarding Audio ON/OFF
5.  Hide camera covert, Event search & remote playback when site type isn't DVR
6.  Change auto reconnect function (all type can used)
7.  Record to network drive improve.
8.  Improve deinterlace video quality.
9.  Motion detection Setting improvement (video and motion bar refresh rate changed from 1sec to 0.3 sec).
10. Device search improvement (search more devices and items on the list can be sorted).
11. Decode MJPEG and H.264 video improvement.
12. Recording restarts after playback is stopped.
13. Disable change of site name at site tree.
14. Add a message showing a link for downloading codec for AVI file conversion.
15. Clear Image when disconnect site.
16. Health status HDD temperature will show "Not available" when connect to DG8X and DG600(SATA not support).
