FW1.4.3
RELEASE NOTE

[IMPORTANT NOTE]
* FW1.4.3 is compatible with VP40, VP42, VP24 and VP28 capture cards.
* The FW1.4.3 is restricted to use 128MB DOM
* FW1.4.3 is restricted to use wheel mouse, it doesn¡¦t support the old-style mouse
* FW1.4.3 supports GPIO Device and the priority is Serial Port Device >VPMB GPIO > GPIO Card
* VP2X Audio input of FW1.4.3 only accepts active microphone
* The MPEG4 video recording file of FW1.4.3 does not support Step Backward

1. Firmware Filename:               Firmware Size:   Firmware date:
   system.bin.en.143_all               27,869,594      2007/01/12  AM 10:28 
   system.bin.tc.143_all               28,807,070      2007/01/12  AM 10:28               
   system.bin.en.143_all_pal           27,869,184      2007/01/12  PM 06:49
   system.bin.tc.143_all_pal           28,807,245      2007/01/12  PM 06:52
   system.bin.en.143_all_nologo        27,871,788      2007/01/12  PM 07:00
   system.bin.tc.143_all_nologo        28,808,917      2007/01/12  PM 07:01
   system.bin.en.143_all_pal_nologo    27,871,795      2007/01/12  PM 07:03
   system.bin.tc.143_all_pal_nologo    28,808,929      2007/01/12  PM 07:04

2. The DCS file list is as follow
2005/05/02  07:38p   2,067,062	avcodec.dll
2007/01/30  01:50p   274,432	DVRPlay.exe
2007/01/02  03:15p   106,560	NPPlayer.exe
2001/12/13  10:47a   217,088	npwmado0.dll
2007/01/02  11:36a   282,624	npwmh263.dll
2007/01/02  11:44a   282,624	npwmjpg.dll
2007/02/07  03:18p   720,896	npwmlavc.dll
2007/01/02  11:47a   913,408	npwmskl4.dll
2007/01/02  11:52a   618,496	npwmxvd4.dll
2004/05/04  07:14p   380,928	VPONAdo.dll
2007/01/31  04:57p   282,624	VPONADO4.dll
2007/02/01  01:28p   397,312	VPONAUD4.dll
2007/02/01  02:28p   630,784	VPONLV.dll
2007/01/30  11:20a   708,608	VPONLV4.dll
2007/02/07  03:29p   983,040	VPONRP4.dl
2007/02/01  02:49p   208,896	VPSCTL.dll
2007/02/01  02:49p   270,336	VPSDEC.dll

3. Driver Version:
	1.1.5

4. Kernel Version:
	2.4.31

[NEW FEATURES]
1.Improvement of MPEG4 Frame Size.
2.Alarm Send Mail function can be configured to send the email at an interval time.
3.Renew Daylight Saving Time. (Due to the changes of Daylight Saving Time of United States).
4.Add the new Chinese font. (Solve the problem of the shortage of words for the old font).
5.System Info may demonstrate DOM Size.
6.System Info may demonstrate Kernel Version.
7.Setup the registration server function can demonstrate the registration result.
8.The DCS acceleration installation and the execution speed (According to the different OS version, it will install different execution files).
9.When GUI mode Live changes to single screen, it can play audio at the same time.
10.When set the record schedule to ¡§motion detection¡¨ or ¡¨motion detection + GPI¡¨, the motion detection will enable automatically.
11.Add the search button to remote playback page and set it to user authority.
12.Support the Gigabit network. (Marvell and Intel Lan Device).
13.Support up to 16 USB PORT Devices.
14.Support up to 16 SCSI HD Devices.
15.Supports SP-Pelco(D) and SP-Pelco(P) PTZ

[BUG FIXED]
1.Fix the reboot problem of changing from 16 split screens to full screen.
2.Fix the problem of Stop Recording. (update bttv driver).
3.Fix the fast playing problem in 4x playback speed mode.
4.Fix the error of Watermark Check Result.
5.Fix the problem of failed configuration of Modem Initial String from web.
6.Support IE7 and fix the error of Remote Download.
7.Fix the IE error problem when operation the step backward function from remote player(DCS).
8.The D01 files are unable to link the execution files automatically from remote player(DCS).
9.Revise the problem of the invalid setting of PDA homepage renewing time.
10.Fix the problem of low Thumbnail video quality.
11.Fix the problem that VP-204 can not link to DVR.
12.Fix the problem of the error configuration of local side when setting the remote VP2x Audio from web. 
13.Fix the reboot problem which is produced by playing back to the files which are deleted due to the insufficient disk space.
14.Fix audio problem (update ALSA driver).
15.Fix nVidia VGA card and LCD monitor of FINE will appear "No Support" message.
16.Fix the problem that Panasonic C850 PTZ can not work.


[Known Problem]
1.The sound test of ASUS P5PL2 will cause the acute beeping.
2.When finish burning the CD in the OSD mode, there is no menu on the screen and it seems the system is dead.
3.When playing back file in OSD mode, Channel 1 and 5 has POS transaction data on the 16 split screen. If user changes to the single screen, the POS transaction data will still show on the screen.
4.When playback the d01 files from remote side, the popup of video and the time can not match if user clicks the time bar to review the video at specific time.
5.The motion photo on the remote FTP will be triggered 10 seconds later than practical time. (The trigger object may already disappear from camera.)
6.Video lost message will not disappear.
7.The system will reboot when the resolution is changed from 320*240 to 640*480. The reboot problem will not happened if you install four vp416 cards. It is happened when only installing one 404R card. After rebooting, the configuration is still revised successfully.
8.When enable the POS function of VP204-1, it will interrupt the connection of VP204-1 after setting the POS EVENT. After POS EVENT setting done, please reboot VPON to regain VP204-1 connection.
9.The video is not refreshed when monitoring the live video from web page by using PDA.
10.The end date of Daylight Saving Time in London is not correct.
11.When setting the date to 2007/10/28 on the local side, the timestamp of the files in ftp will show the date as 2006/10/28 if you change the time area to London.
12.When setting the GPI Trigger Recording function, we suggested for one camera, select  normal recording to avoid the recorded data too few and playback may cause system error.