Main | Quick Start Wizard | Documents | Tools | Tips | Utilities
Back to Default Setting After "factory default reset", you will loose all settings you did before. Make sure you have recorded all useful settings. The password of factory deault is null. 1. Hardware Reset While the router is running ( ACT LED blinking ), press the button and hold for more than 5 seconds. The ACT LED begins to blink rapidly, then release the button. The router will restart with the factory default configuration. 2. Software Reset You can also reset router to factory default via Web configurator.
Copyright (c) 2003, DrayTek Corp. All Rights Reserved.