Main | Quick Start Wizard | Documents | Tools | Tips | Utilities
Accept Incoming Fragmented UDP Packets: Some on-line games (for example : Half Life) will use UDP packets with large length to transfer data. It need to be fragmented. As secure firewall, V2600 will reject these kinds of packets to avoid to be attacked by default. You can enable "Accept Incoming fragmented UDP Packet" function to accept these kinds of packets. Then you can play these kinds of on-line games. Of course, it might have some security concern. Advanced Setup >> IP Filter / Firewall Setup >> General Setup
Copyright (c) 2003, DrayTek Corp. All Rights Reserved.