Main | Quick Start Wizard | Documents | Tools | Tips | Utilities
How do I use the public IP if ISP gives me several public IPs? If you can get a ranges of public IPs via PPPoA/PPPoE or MPoA ,you can enable 2nd subnet to let pcs with public IP to access internet behind Vigor2600. Please set one of the public IPs and their subnet mask as below. Then you can set one of the static public IP to a PC on LAN.
Copyright (c) 2003, DrayTek Corp. All Rights Reserved.