The following procedures will instruct you to install EXSYS PCI MIO
device driver for Windows 3.1

1. Please install EXSYS PCI MIO device driver for DOS first and
   reboot your computer.
2. Use the EXSYS PCI MIO DOS utility --- SHOWMIO.EXE to show up
   the EXSYS PCI MIO adapter configuration (LPTx : I/O address
   and IRQ, COMx : I/O address and IRQ) and write it down.
3. Go into Windows 3.1 ---> Main Group ---> Control Panel --->
   COM Port ---> Select the COMx port ---> Advanced
4. Fill in the Port configuration you just written down (I/O address
   and IRQ).
5. Reboot Windows to make EXSYS PCI MIO device driver for Windows
   3.1 works.

NOTICE:
   Whenever you change any configuration of your computer, you must
   do the above steps again to make EXESYS PCI MIO work properly.


